---
title: Addressing and Connectivity Overview
canonical_url: 'https://docs.projectcalico.org/v1.6/reference/addressing'
---


This diagram shows elements of a Calico network in a simplified way that
allows us to focus on how IP addresses are assigned to workloads, and
whether and how workloads have connectivity to and from the Internet (as
well as to other workloads within the data center).

![]({{site.baseurl}}/images/calico-connectivity.png)

## Network provisioning and IP addresses

In current Calico, the ranges from which IP addresses may be assigned to
workloads are all provisioned by the data center operator. These ranges
are all shared, in the sense that IP addresses from them might be
allocated to workloads for different tenants, and the overall IPv4 and
IPv6 address spaces are 'flat', in that any IPv4 address can in
principle - meaning subject to security policy - communicate with any
other IPv4 address, and similarly for IPv6.

Within the shared address spaces there may be ranges of IP addresses
(both v4 and v6) that are routable from outside the data center. Other
shared network IP address ranges will not be routable from outside: they
are potentially accessible from all other workloads within the data
center, but not from the Internet. This is all under the control of the
data center operators, as it is they who provision the shared network.

## Outbound and inbound connectivity to and from the Internet

Subject to security configuration, *all* forms of IP addressing can
initiate *outbound* connections to outside the data center. In the IPv4
case, the border gateway must NAT the source address of outbound
packets, so that responses to them are routed back to the data center.

In the diagram above, 10.65/16 and 2001:db8:a41:2/64 are IPv4 and IPv6
subnets that are not routable from outside the data center, and
102.25.78/24 and 2001:cf2:45:1/64 are subnets that *are* routable from
outside. For a workload to be accessible from outside the data center,
it simply needs one of its vNICs to be given an IP address from one of
the externally routable ranges.

The following table summarizes the properties of the IP addresses in the
diagram.

| IP address              | Routable from Internet?    | Can access Internet?    |
|-------------------------|----------------------------|-------------------------|
|              10.65.0.18 | No                         | Yes                     |
|      2001:db8:a41:2::12 | No                         | Yes                     |
|             102.25.78.2 | Yes                        | Yes                     |
|       2001:cf2:45:1::3a | Yes                        | Yes                     |
